|  |  |
| --- | --- |
| **Don Declore – Millstone 2** | * First success - PZR spray line has permanent shielding (1/2” Silflex) built into insulation
* 75% reduction in dose rates
* ~35% of Spray Line
 |
| **Dan Stoltz – ANO-2** | * First success –Safety Injection Check Valve (2ST-15) disc replacement. Hydraulic press to push shaft out (time savings)
 |
| **Dan Whisler – Ft Calhoun** | * First success –Smitty Shields
* Second success – Maintenance using RMS for place keeping
 |
| **Lori Grusecki – Palo Verde** | * First success – Aux bldg has excel scaffold permanent installation bolted.
* Second success – Worker engagement dose ownership
 |
|  |  |

|  |  |
| --- | --- |
| **Don Declore – Millstone 2** | * First challenge – High scaffold dose (16 Rem)
 |
| **Dan Stoltz – ANO-2** | * First challenge – Fukeshima mods 2.5 Rem
* Second challenge – Fleet dose management
 |
| **Dan Whisler – Ft Calhoun** | * First challenge – Recovery from flooding
 |
| **Lori Grusecki – Palo Verde** | * First Challenge – Plan for start up crud burst (flush in SDC no longer allowed)
 |

Golden Nuggets:

* + **Millstone 2 – Valve book (Locations, photos, surveys, dose estimates, RWP, and AP)**
	+ **Fort Calhoun – Fire watches with RMS**
	+ **ANO – Hone of pipe preps**
	+ **Palo Verde -**